{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Blad1","Blad2","Blad3"],"not_rendered":{"charts":0,"images":6,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Blad1","index":0,"n_rows":62,"n_cols":21,"rows_kept":62,"cut":false,"hidden":false,"merged":[[18,7,19,7],[19,9,19,10],[18,9,18,10]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," WP 2","Bilaga B"]
[null,null,null,null,null,null,null,"5a","Dimensioneringssystem för naturstenshällar",null,null,null,null,null,null,null," ","       Grågröna systemlösningar för hållbara städer"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"     Obundet bärlager. ",null,"Sätt-och fogsand enl. Utemiljö "]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Brottlast",null,"OBS"]
[null,null,null,null,null,null,null,"t    =",{"$f":"SQRT(1500*I24*I28*I32/I30/I26)","v":{"$error":"#DIV/0!"}},"mm",null,"Trafikklass","KN",null,"Sättsandstjocklek "]
[null,null,null,null,null,null,null,null,null,null,null,"G",3.5,null,"30 mm"]
[null,null,null,null,null,null,null,"P",0,"kN",null,"GC",6]
[null,null,null,null,null,null,null,null,null,null,null,0,9]
[null,null,null,null,null,null,null,"Rtf",0,"MPa",null,1,14]
[null,null,null,null,null,null,null,null,null,null,null,2,25,null,null,null,"Siktkurva för sättning av hällar och gatsten enl Utemiljö "]
[null,null,null,null,null,null,null,"L",0,"mm",null,null,null,null,null,null," I AMA 10 o 13 har siktkurvan  ändrats  utan stenbranschens åsikter"]
[null,null,null,null,null,null,null,null,null,null,null,"Säkerhetsfaktor  EN 1341 (2002)*"]
[null,null,null,null,null,null,null,"W",0,"mm",null,null,"Obundet i sand",null,"* Senare standard från 2012 har andra värden, "]
[null,null,null,null,null,null,null,null,null,null,null,null,"1,6*",null,"     men erfarenhet indikerar att säkerhetsfaktor 1,6 är tillräcklig "]
[null,null,null,null,null,null,null,"Fs",1.6]
[]
[null,null,null,null,null,null,null,"      Slitlagrets totala tjocklek",null,null,{"$f":"(I22+30)","v":{"$error":"#DIV/0!"}},"mm"]
[]
[]
[]
[null,null,null,null,null,null,null,"5b","Dimensioneringssystem för smågatsten "]
[]
[null,null,null,null,null,null,null,"Standardtjocklek på smågatstenen c:a 100 mm"]
[]
[null,null,null,null,null,null,null,"Sättsand c:a 50 mm",null,null,null,null,null,null,null,null,"ca 50 mm"]
[]
[null,null,null,null,null,null,null,"Klarar alla trafikklasser"]
[]
[null,null,null,null,null,null,null,"Slitlagrets totala tjocklek",null,null,150,"mm"]
[]
[]
[]
[null,null,null,null,null,null,null,"5c","Dimensioneringssystem för storgatsten "]
[]
[null,null,null,null,null,null,null,"Standardtjocklek på smågatstenen c:a 140 mm"]
[]
[null,null,null,null,null,null,null,"Sättsand c:a 50 mm",null,null,null,null,null,null,null,null,"ca 50 mm"]
[]
[null,null,null,null,null,null,null,"Klarar alla trafikklasser"]
[]
[null,null,null,null,null,null,null,"Slitlagrets totala tjocklek",null,null,190,"mm"]
[]
[]
[]
[null,null,null,null,null,null,null,"Kurt Johansson    2014-11-30"]

{"sheet":"Blad2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Blad3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}