{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Blad1"],"not_rendered":{"charts":0,"images":4,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Blad1","index":0,"n_rows":48,"n_cols":31,"rows_kept":48,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[null,"Förenklad dimensioneringsberäkning av överbyggnad för trafikklass G/C, 0, 1 och 2 i urban miljö",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," WP 2 x ",null,"Bilaga A"]
[null,"Beläggning med markbetong , natursten  och marktegel. Halvelastisk beläggning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Grögröna systemläsningar för hållbara städer"]
[null,"I bärlager  används samkross  0/32 -  0/40 ",null,null,null,null,null,null,null,"I förstärkningslagret 0/92 -  0/100"]
[]
[null,"        1.Trafikklass",null,"Bär-","  >→","2. Terrassmaterial",null,null,null,"3. Förstärkningslager (0/100)",null,null,null,null,null,null,"  >→"," 4. Klimatzon",null," >→",null,"5. Tjälklass, klimat",null,null,null,"  >→","6. Slitlager och ",null,null," >→","7. Överbyggnad "]
[null,null,null,"lager",null,null,null,null,null,"Terrassmaterial  → tjocklek mm",null,null,null,null,null,null,null,null,null,null,null,"koll o korrigering",null,null,null,null,"sättsandslager ",null,null,null,"Koll o korr"]
[null,null,null,"mm",null,"        Materialtyp→",null,null,1,2,null,3,null,4,null,5,null,null,null,null,"    Total överbyggnadstjocklek",null,null,null,null,null,"Form, tjocklek"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"    se karta",null,null,"    med hänsyn till tjällyftning"]
[null,null,"    G/C ",80,null,"    G/C ",null,null,"30*","80*",null,"80*",null,"80*",null,"180*",null,null,null,null,"Tjälkl","           Klimatzon",null,null,null,null,"Enligt "]
[null,null,0,80,null,0,null,null,"30*","100*",null,"100*",null,210,null,300,null,null,null,null,null,"1     2",3,4,5,null,"tillverkarnas "]
[null,null,1,80,null,1,null,null,"70*","150*",null,240,null,270,null,400,null,null,null,null,3,null,200,375,1150,null,"rekommendation"]
[null,null,2,80,null,2,null,null,"80*","190*",null,270,null,310,null,440,null,null,null,null,4,null,545,1000,1250]
[null,null,null,null,null,"ökning  om  ej krossmatr",null,null,0,0.25,null,0.25,null,0.5,null,0.5,null,null,null,null,null," ur Teknisk rapport, KTH 1999 och Tekniskt PM Scandiaconsult 2002"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"*Om förstärkningslagret < 200  använd samma  material som i bärlagret men komprimeras separat."]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1. Trafikklass",null,null,null,null,null," "]
["Excell beräkning ",null,null,"Överbyggnad",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6.  Slitlager"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6.  Sättlager. Fogmaterial"]
["1. Trafikklass",null,null,"mm"]
[null,"↓",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     Obundet bärlager 80mm"]
["   Bärlagertjocklek",80,"    >→",80]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3. Förstärkningslager"]
["2. Terrassmaterial  ",null,null,"+",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 . Förstärkningslager justering"]
[null,"↓",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," p.g.a.","klimatzon & tjälklass"]
["3. Förstärkningslager",null,"    >→",{"$f":"(B31)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2. Terrass"]
[null,null,null,"  +"]
["6. Slitlager+sättlager",null,"    >→",{"$f":"(B33)","v":0}]
[null,null,null,"  ="]
["Summa överbyggnad",null,null,{"$f":"(D27+D31+D33)","v":80},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5a"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Klimatzoner"]
["5a. Klimatzon"]
[null,"↓"]
["5b. Tjälklass"]
[null,"↓"]
["5. Just. överbyggnad",null,"    >→",{"$f":"(B41)","v":0}]
[null,null,null,"↓"]
["7. Justerart förstärkl.",{"$f":"(D41-D27-D33)","v":-80},"  ←<"]
[]
[]
["Förstärkningslager",{"$f":"(D31)","v":0}]
["tjocklek <200 →0/40 frakt "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"©Kurt Johansson 2016-09-22"]