{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Blad1"],"not_rendered":{"charts":0,"images":4,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Blad1","index":0,"n_rows":45,"n_cols":33,"rows_kept":45,"cut":false,"hidden":false,"merged":[[1,1,1,22],[1,25,1,31],[6,22,6,24]]}
[]
[null,"Förenklad dimensioneringsberäkning av överbyggnad för trafikklass G, G/C, 0, 1, 2 i urban miljö",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dimensionering Urban Överbyggnad  ",null,null,null,null,null,null," Bilaga A"]
[null,null," Beläggning med markbetong , natursten  och marktegel. Halvelastisk beläggning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"        Dimensioneringsmall","Sammanställningsblad"]
[]
[]
[null,null,"1.Trafik",null,"Bär-",null,"2. Terrass",null,null,null,"3. Förstärkningslager (0/100)",null,null,null,null,null,null,null," 4. Klimatzon",null,null,null,"5. Tjälklass, klimat",null,null,null,null,null,"6. Slitlager och ",null,null,null,"7. Kontroll och"]
[null,null,"klass",null,"lager",null,"       materialtyp",null,null,"Terrassmaterial  → tjocklek mm",null,null,null,null,null,null,null,null,null,null,null,null,"koll & korrigering",null,null,null,null,null,"sättsandslager ",null,null,null,"ev. korrigering"]
[null,null,null,null,"mm",null,null,null,null,1,2,null,3,null,4,null,5,null,null,null,null,"Total överbyggnadstjocklek med ",null,null,null,null,null,null,"Form, tjocklek",null,null,null,"av beräkningen"]
[null,null,"G",null,80,null,"G",null,null,0,0,null,0,null,"30**",null,"70*",null,"    se karta",null,null,"hänsyn till tjällyftning. Alla trafikklasser"]
[null,null,"    G/C ",null,80,null,"    G/C ",null,null,"30**","80*",null,"80*",null,"80*",null,"180*",null,null,null,null,"Tjälklass","           Klimatzon",null,null,null,null,null,"Enligt "]
[null,null,0,null,80,null,0,null,null,"30**","100*",null,"100*",null,210,null,300,null,null,null,null,null,"1     2",3,4,5,null,null,"tillverkarnas "]
[null,null,1,null,80,null,1,null,null,"70*","150*",null,240,null,270,null,400,null,null,null,null,3,null,200,375,1150,null,null,"rekommendation"]
[null,null,2,null,80,null,2,null,null,"80*","190*",null,270,null,310,null,440,null,null,null,null,4,null,545,1000,1250]
[null,null,null,null,null,null,"ökning  om  ej krossmaterial",null,null,0,0.25,null,0.25,null,0.5,null,0.5,"Svensk Markbetong: Beläggning med plattor och marksten av betong (2002)"]
[null,null,null,null,null,null,"*Förstärkningslagret < 200  används samma  material som i bärlagret, men packas separat"]
[null,null,null,null,null,null,"**Samma  material som i bärlagret, packas tillsammans med detta"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"             Excelberäkning ",null,null,"Överbyggnad"]
[null,null,null,null,"mm",null,"                  Urban överbyggnad",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"  Klimatzoner"]
[null,"  1.   Trafikklass",2]
[]
[null," Bärlagertjocklek",null,null,80]
[null,null,"↓"]
[null,"2. Terrassmaterial  ",5,null,"+"]
[null,null,"↓"]
[null,"3. Förstärkningslager",440,null,{"$f":"(C27)","v":440}]
[null,null,null,null,"  +"]
[null,"6. Slitlager+sättlager",110,null,{"$f":"(C29)","v":110}]
[null,null,null,null,"  ="]
[null,"Summa överbyggnad",null,null,{"$f":"(E23+E27+E29)","v":630}]
[]
[null,"4. Klimatzon",4]
[null,null,"↓"]
[null,"5. Tjälklass",4]
[null,null,"↓"]
[null,"5. Just. överbyggnad",1000]
[]
[null,"7 a Justerat förstärklag.",{"$f":"(C37-E31)","v":370}]
[null,"7. Justerat förstärkl."]
[null," 0 om 7a neg",370]
[]
[null,"Förstärkningslager",null,null,{"$f":"(E27+C41)","v":810}]
[null,"tjocklek <80 →0/32fraktion ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"                 Version 2018-03-05"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"©Kurt Johansson 2016-09-22"]